PLANET Voice over IP product Firmware/utility Release
--------------------------------------------------

Product supported :      VGW-400 Series
Release date:  	         2014/04/15
New Release Version:     v.140411a
Previous Release:        v.140320c

*** v.140320c
[Issue Fixed]
Increase the outgoing digital limited form 19 digitals to 30 digitals


*** v.140320c
[Add New Function]
1. Add configuration upload page

[Issue Fixed]
1. FXS setting / other page can¡¦t apply
2. FXS port call transfer will fail.
3. VGW-400 series not response the proxy server re-invite message 


*** v140122a
1. Add the delay dialing function in Digit Manipulation
2. Increase the digital length to 64 for all line and sip trunk  user id/ display name /password /tel no / proxy server / domain name /outbound proxy


*** v131023c
1. Initial Release


Upgrade Method
===========
To upgrade the firmware of your router, please logon machine and click on the "Firmware Update" menu. In "Firmware Update" menu, choose "Import" page.
In this page. You can also use the Browse button to allocate the firmware file on your PC. Once the new firmware file is selected, click "Upload" to start the upgrade process. 


Note:
=====
1. Do not turn the power off during the upgrade process. This will damage the unit.
2. Do not upload different model's software. This will damage the unit.
3. File name must be "bin", if change the file format it may damage the system. 



Thanks for choosing PLANET products.


Best Regards ,


PLANET Tech SupportTeam

VoIP Technical Service: support_voip@planet.com.tw