Industrial Dual Band 802.11ax 1800Mbps Wireless Access Point with 5 10/100/1000T LAN Ports
----------------------------------------------------------------------
Model: IAP-1800AX

===============================
Release date: May 30 , 2023
Release version: v1.0
Filename: IAP-1800AX_v1.2102b230526.bin
File size: 13.4 MB
--------------------------------------------------
Update:
	1. Added support for CloudViewerPro app.
	2. Modified the default connection mode of AP to DHCP.



===============================
Release date: Mar. 7, 2022
Release version: v1.0
Filename: IAP-1800AX_v1.2102b220218.bin
File size: 13.7 MB
--------------------------------------------------

[Initial Release]


Upgrade Method
==============
1. To upgrade the firmware of your AP, please log on to the machine and click on the "Maintenance/Firmware Upgrade" menu. 
2. Then, choose firmware file from host, and press "Upgrade". 
3. On this page, you can use the Browse button to allocate the firmware bin file (e.g. IAP-1800AX_v1.xxxxxxxxxx.bin) on your PC. 
4. Once the new firmware file is selected, please select "Reset Default" to resume to the factory configuration or click the "Upgrade" button to upgrade. 


Thanks for choosing PLANET products. Any comment or feedback will be appreciated.
Please regularly check PLANET website for any newer firmware version.

Sincerely yours,
PLANET Technical Support Team
support@planet.com.tw
http://www.planet.com.tw